**Two Counters Dynamic Arch**

|  |  |  |  |
| --- | --- | --- | --- |
| **Task** | **Periodicity**  **(us)** | **Priority** | **First Delay** |
| Switch\_Task | 4000 | 0 | 0 |
| HUart\_Task | 1000 | 1 | 0 |
| APP\_sendTask | 4000 | 2 | 0 |
| CLcd\_Task | 1000 | 3 | 0 |

**Tick Time = 1 mSec**